**TEMPORARY OVERVOLTAGE PROTECTION SPD. UL 1449 4TH EDITION LISTED, TYPE 1, INOMINAL = 20 KA. INSTALL EXTERNAL TO GEAR. NEMA 4/12 ENCLOSURE. SURGE CURRENT RATING TO BE A TESTED VALUE. 20 YEAR WARRANTY. NETWORK-BASED MONITORING SYSTEM. INSTALLED TESTING WITH A PORTABLE SURGE GENERATOR-TEST SET. RECORD ALL LET-THRU VOLTAGES. SUBMIT A REPORT TO THE ENGINEER. CURRENT TECHNOLOGY SL3 SERIES.**